{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Mere","Enota","","Višina","mm","734","734","734"]
["","","","Širina","mm","870","870","870"]
["","","","Globina","mm","373","373","373"]
["Teža","Enota","","","kg","52","52","52"]
["Kompresor","Type","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","° CDB","-20","-20","-20"]
["","","","Maks.","° CDB","52","52","52"]
["","Gretje","Okolje","Min.","°CWB","-21","-21","-21"]
["","","","Maks.","°CWB","18","18","18"]
["Raven zvočne moči","Hlajenje","","","dBA","62","63","64"]
["","Gretje","","","dBA","62","63","64"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","48","49","50"]
["","Gretje","","Nom.","dBA","48","49","50"]
["Hladilno sredstvo","Tip","","","","R-32","R-32","R-32"]
["","Polnitev","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Polnjenje","","","tCO2Eq","1.05","1.05","1.05"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35","6.35"]
["","Plin","","Zun. premer","mm","9.52","12.7","12.7"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","50","50","50"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 30 m)","0,02 (za dolžino napeljave nad 30 m)","0,02 (za dolžino napeljave nad 30 m)"]
["","Višinska razlika","IU - OU","Maks.","m","30","30","30"]
["Standardni pripomočki","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240"]
["Opombe","","","","","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke"]
["","","","","","(3) - Vsebuje fluorirane toplogredne pline","(3) - Vsebuje fluorirane toplogredne pline","(3) - Vsebuje fluorirane toplogredne pline"]
["Standardni pripomočki","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]