{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Mere","Enota","","Višina","mm","1,680"]
["","","","Širina","mm","930"]
["","","","Globina","mm","765"]
["Teža","Enota","","","kg","183.0"]
["Kompresor","Tip","","","","Hermetično zaprt spiralni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-5.0"]
["","","","Maks.","°CDB","46.0"]
["","Ogrevanje","Okolje","Min.","° CWB","-15.0"]
["","","","Maks.","° CWB","15.0"]
["Raven zvočne moči","Hlajenje","","","dBA","78.0"]
["","Gretje","","","dBA","78.0"]
["Hladilno sredstvo","Tip","","","","R-410A"]
["","Polnjenje","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","9.52"]
["","Plin","","Zun. premer","mm","22.2"]
["","Dolžina cevi","Maks.","OU - IU","m","100"]
["","","Sistem","Brez polnitve","m","30"]
["Standardni pripomočki","Priročnik za namestitev","","","","1"]
["","Priključne cevi","","","","4"]
["Power supply","Faza","","","","3N~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","380-415"]
["Tok - 50 Hz","Maksimalni tok varovalk (MFA)","","","A","25"]
["Opombe","","","","","(1) - Napajalni sklop za notranjo enoto FDQ je ločen"]
["","","","","","(2) - Glejte ločene risbe za električne podatke"]
["Mere","Enota","","Višina","mm","","1680"]
["","","","Širina","mm","","930"]
["","","","Globina","mm","","765"]
["Teža","Enota","","","kg","","184.0"]
["Kompresor","Tip","","","","","Hermetično zaprt spiralni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","","-5.0"]
["","","","Maks.","°CDB","","46.0"]
["","Gretje","Okolje","Min.","° CWB","","-15.0"]
["","","","Maks.","° CWB","","15.0"]
["Raven zvočne moči","Hlajenje","","","dBA","","78.0"]
["","Gretje","","","dBA","","78.0"]
["Hladilno sredstvo","Polnitev","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Polnjenje","","","tCO2Eq","","19.4"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","12.70"]
["","Plin","","Zun. premer","mm","","22.2"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","","100"]
["","","Sistem","Brez polnitve","m","","30"]
["Standardni pripomočki","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Napajanje","Frekvenca","","","Hz","","50"]
["Tok – 50 Hz","Maksimalni tok varovalk (MFA)","","","A","","25"]