{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","SAR"]
[]
[]
[]
[]
["","","","","SAR212DB13SSA","SAR212DB13SSB","SAR320DB13SSA","SAR320DB13SSB","SAR430DB13SSA","SAR430DB13SSB"]
["Ohišje","Barva","Kondenzator","","Bela","Bela","Bela","Bela","Bela","Bela"]
["Mere","Kondenzator","Širina","mm","695","","754","","1280"]
["","","Globina","mm","305","","400","","440"]
["","Uparjalnik","Višina","mm","","280","","450","","450"]
["","","Širina","mm","","720","","720","","1120"]
["","","Globina","mm","","540","","700","","700"]
["Kompresor","Količina","","","1","","1","","1"]
["","Tip","","","Gnani parni kompresor","","Gnani parni kompresor","","Gnani parni kompresor"]
["","Model","","","FH4524Z-XG","","MTZ40JH4","","MTZ64HM4"]
["","Način zagona_","","","Neposredni","","Neposredni","","Neposredni"]
["Kondenzator","Zračni tok","","m³/h","1400","","1500","","2700"]
["Odmrzovanje","","","","Vroči plin","","Vroči plin","","Vroči plin"]
["Delovni doseg","Temperatura hladilnice","Min.","°C","-5","","-5","","-5"]
["","","Maks.","°C","10","","10","","10"]
["Območje delovanja","Temperatura okolice","Min.","°C","20","","20","","20"]
["","","Maks.","°C","45","","45","","45"]
["Hladilno sredstvo","Tip","","","R-452A","","R-452A","","R-452A"]
["","GWP","","","2140","","2140","","2140"]
["Napajanje","Napetost","","V","380-400","","380-400","","380-400"]
["","Faza","","","3N~","","3N~","","3N~"]
["","Frekvenca","","Hz","50","","50","","50"]