{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":7,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","SEHVX-AAW / SERHQ-AAW1"]
[]
[]
[]
[]
["","","","","SEHVX20AAW / SERHQ020AAW1 (Archived)","SEHVX32AAW / SERHQ032AAW1 (Archived)","SEHVX64AAW / SERHQ032AAW1+SERHQ032AAW1 (Archived)"]
["Razpon energetske učinkovitosti","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Hladilna kapaciteta","Nom.","","kW","","","62.3"]
["Vhodna moč","Hlajenje","Nom.","kW","","","27.4"]
["EER","","","","","","2.27"]
["Raven zvočne moči","Hlajenje","Nom.","dBA","","","83"]
["Opombe","","","","","","(1) - Gretje Ta DB/WB 7/6°C - LWC35°C (DT = 5°C), podatki v skladu z EN 14511: 2011"]
["","","","","","","(2) - Gretje Ta DB/WB 7/6°C - LWC45°C"]
["","","","","","","(3) - Hlajenje: Ta 35°C - LWE 7°C (DT=5°C), podatki v skladu z EN 14511: 2011"]
["","","","","","","(4) - Delovanje odvisno od fluoriranih toplogrednih plinov"]