{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Tiho delovanje","dBA","","36","","41"]
["","","","Nizko","dBA","","38","","43"]
["","Hlajenje","","Tiho delovanje","dBA","","36","","41"]
["","","","Nizko","dBA","","38","","43"]
["","","","Visok","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Standardni pripomočki","Priročnik za namestitev","","","","","Priročnik za namestitev","","Priročnik za namestitev"]
["","Priročnik za upravljanje","","","","","Priročnik za upravljanje","","Priročnik za upravljanje"]
["","Vijaki","","","","","Vijaki","","Vijaki"]
["","Podložka","","","","","Podložka","","Podložka"]
["","Brezžičen daljinski upravljalnik","","","","","Brezžičen daljinski upravljalnik","","Brezžičen daljinski upravljalnik"]
["","Pokrivna zaporna mreža","","","","","Pokrivna zaporna mreža","","Pokrivna zaporna mreža"]
["","Baterija","","","","","Baterija","","Baterija"]
["Krmilni sistemi","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrard. dalj. krm.","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Liquid","","OD","mm","","9.52","","9.52"]
["","Plin","","OD","mm","","15.88","","15.88"]
["","priključka","","","","","19.05","","19.05"]
["Power input","Hlajenje","","Nom.","kW","","0.094","","0.137"]
["","Gretje","","Nom.","kW","","0.094","","0.137"]
["Raven zvočne moči","Hlajenje","","","dBA","","56","","60"]
["","Gretje","","","dBA","","56","","60"]
["Mere","Enota","","Width","mm","","820","","820"]
["","","","Depth","mm","","820","","820"]
["","","","Višina","mm","","300","","300"]
["Ohišje","Material","","","","","Galvanizirano jeklo","","Galvanizirano jeklo"]
["Teža","Enota","","","kg","","39","","39"]
["Ventilator","Hitrost pretoka zraka","Ogrevanje","Visok","m³/min","","29.2","","34.0"]
["","","","Nizko","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Hlajenje","Nizko","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Visok","m³/min","","29.2","","34.0"]
["","","","Tiho delovanje","m³/min","","17.6","","22.1"]
["","","Hlajenje","Tiho delovanje","m³/min","","17.6","","22.1"]
["Okrasna plošča","Teža","","","kg","","4","","4"]
["","Mere","","Višina","mm","","82","","82"]
["","","","Globina","mm","","990","","990"]
["","","","Širina","mm","","990","","990"]
["","Barva","","","","","Bela","","Bela"]
["Power supply","Faza","","","","","1~","","1~"]
["","Ime","","","","","V1","","V1"]
["","Frekvenca","","","Hz","","50","","50"]
["","Napetost","","","V","","220-240","","220-240"]
["Ventilator","Hitrost pretoka zraka","Gretje","Tiho delovanje","m³/min","15","","22.1"]
["Vhodna moč","Gretje","","Nom.","kW","0.067","","0.137"]
["","Hlajenje","","Nom.","kW","0.067","","0.137"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Tiho delovanje","m³/min","15","","22.1"]
["Ohišje","Material","","","","Galvanizirano jeklo","","Galvanizirano jeklo"]
["Mere","Enota","","Višina","mm","265","","300"]
["","","","Širina","mm","820","","820"]
["","","","Globina","mm","820","","820"]
["Teža","Enota","","","kg","31","","39"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Nizko","m³/min","17.6","","26.3"]
["","","Gretje","Visok","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Nizko","m³/min","17.6","","26.3"]
["Raven zvočne moči","Hlajenje","","","dBA","54","","60"]
["","Gretje","","","dBA","54","","60"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Nizko","dBA","35","","43"]
["","","","Tiho delovanje","dBA","32","","41"]
["","Gretje","","Visok","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Nizko","dBA","35","","43"]
["","","","Tiho delovanje","dBA","32","","41"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","9.52","","9.52"]
["","Plin","","Zun. premer","mm","15.88","","15.88"]
["","Izpust","","","","19.05","","19.05"]
["Okrasna plošča","Mere","","Višina","mm","82","","82"]
["","","","Širina","mm","990","","990"]
["","","","Globina","mm","990","","990"]
["","Teža","","","kg","4","","4"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARCWLA","","ARCWLA"]
["","Ožičeni daljinski krmilnik","","","","ARCWB","","ARCWB"]
["Standardni pripomočki","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Napajanje","Faza","","","","1~","","1~"]
["","Frekvenca","","","Hz","50","","50"]
["","Napetost","","","V","220-240","","220-240"]