{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.020"]
["","Gretje","","Nom.","kW","0.020"]
["Ohišje","Barva","","","","Črna"]
["Mere","Enota","","Višina","mm","295"]
["","","","Širina","mm","798"]
["","","","Globina","mm","189"]
["Teža","Enota","","","kg","11.5"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","11.0"]
["","","","Srednja","m³/min","8.2"]
["","","","Nizko","m³/min","6.1"]
["","","","Tiho delovanje","m³/min","4.6"]
["","","Gretje","Visok","m³/min","10.9"]
["","","","Srednja","m³/min","8.7"]
["","","","Nizko","m³/min","6.4"]
["","","","Tiho delovanje","m³/min","4.5"]
["Sound power level","Hlajenje","","","dBA","57"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","39"]
["","","","Srednja","dBA","32"]
["","","","Nizko","dBA","25"]
["","","","Tiho delovanje","dBA","21"]
["","Gretje","","Visok","dBA","39"]
["","","","Srednja","dBA","32"]
["","","","Nizko","dBA","25"]
["","","","Tiho delovanje","dBA","21"]
["Hladilno sredstvo","GWP","","","","675.0"]
["Priključki napeljave","Tekočina","","Zun. premer","mm","6.35"]
["","Plin","","Zun. premer","mm","9.50"]
["","priključka","","","","18"]
["Krmilni sistemi","Infrared remote control","","","","ARC466A85"]
["","Wired remote control","","","","BRC073A1"]
["Standardni pripomočki","Priročnik za namestitev","","","","1"]
["","Priročnik za upravljanje","","","","1"]
["","Zračni filter","","","","2"]
["","Infrardeči daljinski upravljalnik","","","","1"]
["","Montirna plošča daljinskega upravljalnika","","","","1"]
["","Vrečka vijaka","","","","1"]
["","Vijačni pokrov","","","","2"]
["","Suhe baterije AAA","","","","2"]
["","Splošni varnostni previdnostni ukrepi","","","","1"]
["Power supply","Ime","","","","V1"]
["","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]