{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTP-N8"]
[]
[]
[]
[]
["","","","","","RXTP25N2V1B8","RXTP35N2V1B8"]
["Raven zvočnega tlaka","Gretje","","Nom.","dBA","49","49"]
["","Hlajenje","","Nom.","dBA","48","48"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","1"]
["","Oznaka polnitve hladilnega sredstva","","","","1","1"]
["","Večjezikovne oznake za fluorirane toplogredne pline","","","","1","1"]
["Hladilno sredstvo","Charge","","","TCO2Eq","0.75","0.75"]
["","GWP","","","","675","675"]
["","Polnitev","","","kg","1.1","1.1"]
["","Tip","","","","R-32","R-32"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","450","450"]
["","","Gretje","Izjwemno nizka","vrt/min","360","360"]
["Piping connections","Višinska razlika","IU - OU","Maks.","m","15","15"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)"]
["Kompresor","Type","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Mere","Enota","","Širina","mm","763","763"]
["","","","Globina","mm","312","312"]
["","","","Višina","mm","551","551"]
["Teža","Enota","","","kg","38","38"]
["Power supply","Phase","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-240","220-240"]
["Opombe","","","","","(1) - Vsebuje fluorirane toplogredne pline","(1) - Vsebuje fluorirane toplogredne pline"]
["","","","","","(2) - Glejte ločeno risbo za obratovalno območje","(2) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(3) - Glejte ločeno risbo za električne podatke","(3) - Glejte ločeno risbo za električne podatke"]